BLUE "Q"   Installation Instructions...

•	Directions:  inject in compressor oil reservoir or in low pressure return side of refrigerant flow line.  Should be injected by qualified technician using proper equipment.  Store at room temperature in container tightly closed, keep clean, dry and away from open flame...

•	Dosage = for equipment "less" than 75 tons per unit = 1 ounce per TON/HP per unit...

•	Dosage = for equipment  75 - 100 Tons/HP = 3/4 of an ounce per ton

•	Dosage = for equipment over 100 tons = 1/2 ounce per ton per unit...

Any questions, Pls contact Dr George - info@energy-group.com   or
                            ( Phone: = 1 - 973 – 942 – 8628 )